Activation: (Kako aktivirati) 

1. Ignition switch on, 
2. "circulating air" key keep pressed 
3. "ventilation nozzles above" - key press 
4. two keys release 
5. In the indication area now "0C" and the Dimmung appear switch on 100% 
6. With the cold/warm keys now the function (Diagnosekanal)gewaehlt can become, 
7. Channel with "circulating air" confirm 
8. Deactivation over "car" 


Channel/contents (Kanali) 

1 system error 
2 actual value feeler virtually 
3 actual value interior feeler console 
4 actual value outside temperature - feeler wasserkasten 
5 actual value outside temperature - feeler bumper 
6 actual value blowing out feeler floor space 
7 actual value blowing out feeler Mannanstroemer 
8 display checks 
9 actual digital value acknowledging potentiometer temperature flap 
10 target digital value temperature flap 
11 actual digital value acknowledging potentiometer A/C flap 
12 target digital value A/C flap 
13 actual digital value acknowledging potentiometer Fuss/Def flap 
14 target digital value Fuss/Def flap 
15 actual digital value acknowledging potentiometer ram air flap 
16 target digital value ram air flap 
17 driving speed (km/h) 
18 actual value of the blower tension (volt) 
19 desired value of the blower tension (volt) 
20 actual value of the generator/on-board tension (volt) 
21 number of low-voltage events (not volatile) 
22 sound condition of the high pressure switch 
23 number of high pressure events (volatile) 
24 number of high pressure events (not volatile) 
25 A/D value kickdown switch 
26 A/D value hot light 
27 engine speed 
28 generator number of revolutions 
29 coding 
30 software-Version 
31 software index 
32 potentiometer error counters temperature flap 
33 potentiometer error counters A/C flap 
34 potentiometer error counters Fuss/Def flap 
35 potentiometer error counters ram air flap 
36 temperature flap notice cold 
37 temperature flap notice warm 
38 A/C flap notice closed 
39 A/C flap notice opened 
40 Fuss/Def flap notice Def 
41 Fuss/Def flap notice foot 
42 ram air flap notice up 
43 ram air flap notice too 
44 operating cycle counters 
45 interior temperature counted (Ninc) dig 
46 outside temperature filtered (°C) 
47 outside temperature not filtered (°C) 
48 ECOR 
49 error counters Tachosignal 
50 service life in min 
51 engine temperature °C 
52 generator Abschall conditions (see appendix) 
53 announcement more actively el. Exits: Generator/circulating air valve/water 
valve 
54 rule index 
55 outside temperature °C 
56 interior feelers virtually °C 
57 interior feelers console °C 
58 temperature wasserkasten °C 
59 temperature bumper °C 
60 blowing out feelers floor space °C 
61 blowing out feelers Mannanstroemer °C 
62 sun intensity W/m-1 
63 sun intensity filtered W/m-1 
64 delta exhaust rise 
65 delta A/C Klappenverschiebung 
66 time constant/1.6 seconds 
67 cold weather starting correction 
68 maximum correcting variable for i and p-portion 
69 actual value blowing out feeler foot (cnts) 
70 desired value blowing out feeler foot (cnts) 
71 deviation (Epsilon) 
72 portion (+ heat/- cool
