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Riese Pio X (Treviso) Italia 13/02/2015

We declare that Arcasting alloy wheels type  D666 with the following specifications:

- Code: A136

- Dimensions : 7,5x18

- ET 35

- PCD 5x110

-Central Bore 65,1

They are produced in our factory which is located in Riese Pio X Via Monte Santo 41 31039 (TV) Italy.

We further declare that the wheels in question have been subjected to the impact test (test SAE J175) and bending moment fatigue test and have passed both tests successfully applying the loads required for the car Opel Astra GTC-OPC Car type A-H/C.

In view of the on written Arcasting authorizes the installation of wheel type D666 7,5x18 et 35 5x110 65.1  on Opel Astra GTC-OPC Car type A-H/C.

Arcasting s.r.l.

Le informazioni contenute nella comunicazione che precede possono essere riservate e sono, comunque destinate esclusivamente alla persona e/o all’ente sopraindicati. La diffusione, distribuzione e/o copiatura del documento trasmesso da parte di qualsiasi soggetto diverso dal destinatario è proibito (d.lgs.. 196/2006). Se avete ricevuto questo messaggio per errore Vi preghiamo di distruggerlo e informarci immediatamente per telefono. Grazie 

The information contained in this letter may be confidential and is, however, intended for the exclusive use of the individual or entity to whom it is addressed. If you receive this letter by mistake, please inform us immediately and destroy it. Disclosure, distribution or copying of this letter maybe subject to legal restriction.
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